Time parameters

# Plug-In "Time parameters"

The plug-In "Time parameters" allows the program to calculate and display duration, duty cycle and frequency of a signal.
Plug-In "Time parameters", mode "pulse width".
This plug-in and mode allows the program to display in real time the pulse width of a signal, for example injector pulse width.
Plug-In "Time parameters", mode "duty cycle and frequency".
This plug-in and mode allows the program to display the duty cycle and frequency of a repetitive signal in real time. When analyzing PWM (Pulse Width Modulation) signals it may be necessary to operate the vehicle in such a manner that the PWM is activated. One example would be the PWM solenoid for the TCC (Torque Converter Clutch) in the transmission.
Plug-in "Time parameters" displays this information for the channel that the oscilloscope is set to trigger from.